/**
 * @defgroup    boards_stm32f746g-disco STM32F746G-DISCO
 * @ingroup     boards
 * @brief       Support for the STM32F746G-DISCO board.

## Flashing the device

The STM32F746G-DISCO board includes an on-board ST-LINK programmer and can be
flashed using OpenOCD.
The board can be flashed with:

```
make BOARD=stm32f746g-disco flash
```

and debug via GDB with
```
make BOARD=stm32f746g-disco debug
```

## Supported Toolchains

For using the STM32F746G-DISCO board we recommend the usage of the
[GNU Tools for ARM Embedded Processors](https://launchpad.net/gcc-arm-embedded)
toolchain.

 */
